     CITY OF FLUSHING - RENTAL HOUSING INSPECTION CHECKLIST – FOR REFERENCE ONLY


SMOKE Detectors: 
☐  Properly installed and operable 
☐  Installed in correct locations: In sleeping units, outside of sleeping units, and on every floor 
FURNACE: 
☐  Gas shut off valve and on/off switch 
☐  Vent secured and properly pitched 
☐  Filters are replaced/cleaned regularly 
☐  Operable, provides minimum 68 degrees  
☐  Adequate surrounding clearance WATER HEATER: 
☐  Gas shut off valve 
☐  Proper pop-off valve and drop line 
☐  Vent secured and properly pitched 
☐  Operable with no rust holes or leaks 
☐  Adequate surrounding clearance 
ELECTRICAL PANEL:
☐  Service amps adequate for usage 
☐  Properly grounded and in good condition 
☐  No open circuits in box 
☐  All circuits labeled and readable 
☐  If fuses – proper sizes 
☐  Adequate clearance and easy access
 GENRAL ELECTRICAL: 
☐  Covers on switches, junction boxes and outlets 
☐  Splices to code in covered boxes 
☐  Wire in conduit where required 
☐  GFCIs where required and operable 
☐  Switches, outlets, and fixtures operable 
☐  Minimum 2 outlets in all rooms, properly spaced 
☐  Adequate light fixtures, with globes as required 
☐  Buffer space between lights and combustibles 
☐  Safe, limited use of extension cords 
☐  Exterior service lines secure and protected 
GENERAL PLUMBING: 
☐  Installed correctly with no leaks 
☐  Proper venting 
☐  Functioning drains with proper traps and covers SINKS, BATHTUBS & SHOWERS: 
☐  Ventilation in bathroom 
☐  Proper number and location 	 
☐  Operable, with hot and cold water 
☐  Functioning drains with proper traps 
☐  No leaks or drips 
☐  Garbage disposal operable if present TOILETS: 
☐  Operating properly 
☐  No overflow to sewer from tank 
☐  No leaks or continuous running LAUNDRY: 
☐  Proper dryer vent to exterior with cover 
☐  Gas shut off valve, end of line capped if unused 
☐  Proper and grounded electrical connection 
☐  Washtub faucet backflow prevention present 



WINDOWS: 
☐  Proper location and sizes for light and ventilation 
☐  Proper for egress and lockable 
☐  Snug fit, openable and not broken or cracked 
☐  Screens installed between June 1 and October 15 
☐  Egress windows for basement bedrooms 
☐  Bathrooms have operable window with screen (June 1-Oct. 15) or a vent fan 
DOORS:  
☐  Bedrooms and bathrooms require privacy doors 
☐  Bedroom doors – no padlocks or inside keyed 
☐  Exterior doors – correct for egress and lockable 
☐  Exterior doors – snug fit, operable and unbroken 
ROOMS: 
☐  Walls, floors, and ceilings intact and maintained 
☐  Unobstructed egress within and out of home 
☐  Proper square footage, ceiling height and layout 
☐  Fireplaces, wood stoves operable and maintained 
☐  No rubbish or garbage accumulation, infestations 
☐  Basement bedrooms comply with all safety codes 
STAIRWAYS: 
☐  Adequately lighted, no stored items blocking egress 
☐  Steps stable, unbroken and adequate strength 
☐  Handrails required if 5 or more steps 
☐  Guardrails on open stairs over 30” high 
BUILDING EXTERIOR: 
☐  Roof waterproof and maintained; gutters work 
☐  Walls, foundation, and chimney maintained 
☐  Porches solid and maintained 
☐  No openings for animal infestations 
☐  Guardrails on porches or stairs over 30” high 
☐  Handrails required if 5 or more steps 
☐  House numbers present and readable from street 
GARAGE: 
☐  Proper electrical service, wiring, fixtures, etc. 
☐  Structure solid and maintained YARD: 
☐  Fences built to code and maintained 
☐  Grass, shrubs, and trees maintained to code   
☐  Accessory buildings maintained to code 
☐  Pools maintained and secure from child entry 
☐  Outdoor trash kept in solid covered container 
☐  No junk, trash, or building materials stored outside 
☐  No inoperable vehicles or stored vehicle parts/tires 
☐  No improper vehicle, RV or trailer parking 
☐  No unsafe or unsanitary conditions 
☐  Pet waste must be removed regularly 
GENERAL: 
☐  Permits pulled for repairs or new work required 
 
Note: It is REQUIRED that a fire extinguisher be provided for safety. City of Flushing rental inspections do not include inspections for mold, airborne contaminants or other possible contaminants. 
 
Note: This is not a comprehensive list of all requirements. Questions? Please email the Rental Inspection Department at rentalinspections@flushingcity.com.
